QWK

Internal ProBoard QWK support has been added! It is provided as a PEX file called QWK.PEX. The only things necessary to configure are the following:

The packet file name your BBS will create (ProCFG/Options/QWK).

The QWK area name in each message area configuration.

Call the QWK PEX as any you would any other PEX file. No configuration files are necessary. One parameter can be given: “D” (ie “QWK D”). This will pack all mail and start the download right away.